**Quotation Call Notice**

Sealed quotations are invited from registered **Firms/Agencies/Supplier** having valid **VAT/TIN/PAN/Registration documents** to supply and install the following items in Central Computer Lab-1 of Computer Science & Engineering Department as specified below:

**Item with Specification Quantity**

1. 32 Chanel HD CVI DVR 01

 Warranty: - 1 Year

1. 1.3 Megapixel HD CVI IR Doom Camera(20mtr) 20

Warranty: - 1 Year

1. 1.3 Megapixel HD CVI IR Bullet Camera(60mtr) 04

Warranty: - 1 Year

1. 2 TB Hard disk(HDD), Warranty: - 1 Year 01
2. VNC Pin 55
3. DC Connector 30
4. 10 Amp power supply, Warranty: - 1 Year 02

**Copper cable with & other required accessories for the proper installation**

**32 Chanel HD CVI DVR: -** Support HDCVI/Analog/IP Video input, All channel 720P Realtime Recording, H.264 dual-stream Video Compression, HDMI / VGA / TV Simultaneous Video Output, Support Multi-brand network cameras, Support 2 SATA HDDs up to 8TB, 2 USB2.0, Mobile Software with CMS Software, Embedded processor, 1920x1080, 1280x1024, 1280x720, 1024x768 Video Resolution, 1 HDMI, 1 VGA, 1 TV Video output, Main Stream: 720P/960H / D1(1-25/30fps), Extra Stream: CIF / QCIF(1-25/30fps) video recording, 1/4/8/9/16/25/36 Video Display Split, Manual, Schedule(Regular(Continuous), MD), Stop in Recording Mode, Play, Pause, Stop, Rewind, Fast play, Slow play, Next file, Previous file,Next camera, Previous camera, Full screen, Repeat, Shuffle, Backup, selection, Digital zoom in Playback, RJ-45 port (10/100M/1000M) for Ethernet.

**1.3 Megapixel HD CVI IR Doom Camera:-**1/2.9" 1.3MP HQIS Pro Image Sensor, 25/30fps@1.3MP, Day/Night(ICR), AWB, AGC, BLC, 3.6mm Lens, IR Range of 20 Mtr, S/N ratio>50db, 1.3MP @25fps for video streaming, 24Nos. of IR LEDs.

**1.3 Megapixel HD CVI IR Bullet Camera(60mtr):-** 1/2.9" 1.3MP HQIS Pro Image Sensor, 25/30fps @1.3MP, Day/Night(ICR), AWB, AGC, BLC, 12mm Lens, IR Range of 60 Mtr., IP66, 1/60-1/100,000sec shutter speed, 12mm lens>50db s/n ratio, 1.3mp@25fps for video streaming, 1.0vp-p75 for video output, 195mm x 125mm x 110mm in dimension, 4 pcs array for IR LEDs.

**2 TB Hard disk(HDD):-** Seagate, Samsung, Fujistu, Hitachi, Sony. **Copper VNC Pin.**

The cost of the above mentioned items along with make and model no should be quoted individually. The intenders are required to submit the offer along with the VAT/TIN/PAN/Registration certificates. The Firms/Agencies should write quotations for “Supply & Installation of CCTV Surveillance system in CCL-1” in bold letters on covered envelops. The firm should not be black listed during last three financial years.

 The last date submission of quotations is **30.11.2016** up to 3.00 PM addressing to the **Principal, College of Engineering and Technology, Techno Campus, MahalaxmiVihar,Bhubaneswar-29** by speed post/Registered post/Courier only. No hand delivery is accepted. The authority will not responsible for any postal delay.

The authority reserves the right to reject any or all quotations without assigning any reason thereof.

 Sd/-

PRINCIPAL