**Quotation Call Notice**

Sealed quotations are invited from registered **Firms/Agencies/Supplier** having valid **VAT/TIN/PAN/Registration documents** for supply and installation of the following items in Central Computer Laboratory-II managed by IT Department as specified below:

|  |  |
| --- | --- |
| **Item with Specification** | **Quantity** |
| 1. 12 Volt 26AH Battery with Rack compatible to 10 KVA online UPS of EATON make

(On Buy back of Twenty (20) nos of old 12Volt 7AH battery of Rocket make) | **20 Nos** |
| 1. AMC for one number of EATON make 10KVA online UPS

(Authorisation certificate from EATON is a must) | **01 No** |

The cost of the above mentioned items along with make and model no should be quoted individually. The intenders are required to submit the offer along with the VAT/TIN/PAN/Registration certificates. The Firms/Agencies should write quotations for **“Supply and installation of Twenty (20) nos of 12 Volt 26AH Battery and AMC for EATON make 10KVA online UPS of Central Computer Laboratory-II.”** in bold letters on covered envelops. The firm should not be black listed during last three financial years.

 The last date submission of quotations is **22/12/2016** up to 3.00 PM addressing to the **Principal, College of Engineering and Technology, Techno Campus, Mahalaxmi Vihar, Ghatikia, Bhubaneswar-29** by speed post/Registered post/Courier only. No hand delivery is accepted. The authority will not responsible for any postal delay.

The authority reserves the right to reject any or all quotations without assigning any reason thereof.

Sd/-

Principal

**Quotation Call Notice**

Sealed quotations are invited from authorized Electrical Contractor or equivalent Firms/Agencies having valid **VAT/TIN/PAN/Registration documents for** supply and install the following items in Central Computer Laboratory-II managed by IT Department as specified below:

|  |  |
| --- | --- |
| **Item with Specification** | **Quantity** |
| Electrolyte Copper plate Sensitive earthing with excavation of earth pit in all types of soil and Rock of minimum size 4ft X 4ft X 11ft with 600mm X 600mm Electrolyte Copper plate and ISI marked GI pipe of size 1.5” X 10’ long , filling of charcoal, salt and addition of graphite as per suitability. Supply fixing, laying undergrounding of 19 mm X 3mm copper flat from copper plate to top of the earthpit with brass or copper nutbolt and washer etc. The earthing points should be bounded with 4’X4’X3’ bricks wall for identification in future.  | **2 Nos** |
| Supply , fixing, laying, undergrounding of No.8 copper conductor from earth pit to 2nd floor UPS Bus-Bar complete with all fittings. | **60’****(Approximately)** |

The cost of the above mentioned items should be quoted individually. The Warranty period of the above item should be minimum one year from the date of successful installation and performance. The intenders are required to submit the offer along with the VAT/TIN/PAN/Registration certificates. The Electrical Contractor or equivalent Firms/Agencies should write quotations for **“Supply / installation and excavation of Electrolyte Copper Plate sensitive earthing in Central Computer Laboratory-II Department ,CET,BBSR”** in bold letters on covered envelops. The firm should not be black listed during last three financial years.

 The last date submission of quotations is **\_\_\_\_\_\_\_\_\_\_\_** up to 3.00 PM addressing to the **Principal, College of Engineering and Technology, Techno Campus, Mahalaxmi Vihar, Ghatikia, Bhubaneswar-29** by speed post/Registered post/Courier only. No hand delivery is accepted. The authority will not responsible for any postal delay.

The authority reserves the right to reject any or all quotations without assigning any reason thereof.

Principal

Copy to- PIC,CCL-II for information and necessary action