**SHORT TENDER NOTICE FOR COE-AI LAB**

Sealed tenders are invited from OEM, authorized dealer and distributors to supply and install carpet for the COE-AI Lab. approximately 1200 Sq.ft. The last date of submission of Tender is **07.12.2019 by 4:00 PM**. The sealed tender will be received by speed post/ registered post only. No hand or Courier delivery will be accepted. The authority will not be held responsible for any postal delay. Tender received after the scheduled date and time will not be accepted. The tender documents with details of terms and conditions are to be downloaded from the College Website: [**www.cet.edu.in**](http://www.cet.edu.in)**.**

The authority reserves the right to reject/cancel the tenders in whole or in part without assigning any reason thereof.

Sd/-

**PRINCIPAL**

* TECHNICAL SPECIFICATION:-
* Roll type carpet, EUROPEAN Made(Asian make not acceptable). Brand “Carus”, "Aqua" or equivalent suitable & recommended to be used in an Auditorium application.
* The selected carpet should have inbuilt “Scotch guard®” “Type 6 Crealon® Nylon”, and “Weave back®” for better performance.
* Minimum pile height of 7mm, with a total height of 9mm, should also have a minimum pile weight of 800g/m² and a minimum total weight of 1650g/m², to ensure adequate quality for the said usage.
* The carpet should have minimum 185040/m² number of tufts, to ensure good density to perform under heavy traffic usage.
* The carpet should also have color fastness standard of minimum 4 or more for rubbing (wet or dry), water or light. It should also have thermal resistance of 0.072m²K/W and impact sound insulation of minimum 25 or more.

EMD:- DD of Rs.1000/- in favour of Principal, CET,BBSR